<?xml version="1.0"?>
<ProjectConfig xmlns:xsd="http://www.w3.org/2001/XMLSchema" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">
  <Settings>
    <Version>1.1</Version>
    <Affect>Document</Affect>
  </Settings>
  <Config />
  <Documents>
    <DocumentConfig>
      <Name>TRI-SQR-VCO_OTA.SchDoc</Name>
      <Id>CGKTLQAR</Id>
      <Config>OP_Analysis=True|TRAN_Analysis=True|DC_Analysis=True|AC_Analysis=True|TF_Analysis=False|PZ_Analysis=False|Noise_Analysis=False|TRAN_FourierAnalysis=False|TempSweep_Analysis=False|ParamSweep_Analysis=False|MonteCarlo_Analysis=False|TF_Enabled=False|TF_Source=|TF_Reference=0|PZ_Enabled=False|PZ_Node1=|PZ_Node2=0|PZ_Node3=|PZ_Node4=0|PZ_AnalType=PZ|PZ_TfType=VOL|AnalysesDataSavedIndex=4|DC_ShowMeasTableChart=False|DC_PrimarySource=IC1A|DC_PrimaryStart=1n|DC_PrimaryStop=1u|DC_PrimaryStep=100n|DC_EnableSecondary=False|DC_SecondarySource=|DC_SecondaryStart=|DC_SecondaryStop=|DC_SecondaryStep=|Noise_Enabled=False|Noise_Source=|Noise_Output=|Noise_Reference=0|Noise_Start_UserValue=20|Noise_Start=20|Noise_Stop_UserValue=20k|Noise_Stop=20k|Noise_TestPoints_UserValue=10|Noise_TestPoints=10|Noise_PointsPerSummary=0|Noise_SweepType=DEC|AC_StartFrequency_UserValue=20|AC_StartFrequency=20|AC_StopFrequency_UserValue=20k|AC_StopFrequency=20k|AC_TestPoints_UserValue=10|AC_TestPoints=10|AC_SweepType=DEC|AC_ShowMeasTableChart=False|TRAN_StartTime_UserValue=10m|TRAN_StartTime=10m|TRAN_StopTime_UserValue=16m|TRAN_StopTime=16m|TRAN_StepTime_UserValue=1u|TRAN_StepTime=1u|TRAN_MaxStepTime_UserValue=1u|TRAN_MaxStepTime=1u|TRAN_AlwaysSetDefaults=False|TRAN_DefaultCycles_UserValue=5|TRAN_DefaultCycles=5|TRAN_DefaultPointsPerCycle_UserValue=50|TRAN_DefaultPointsPerCycle=50|TRAN_UseInitialConditions=False|TRAN_FourierEnabled=False|TRAN_FourierFundFreq_UserValue=|TRAN_FourierFundFreq=1Meg|TRAN_FourierNumHarmonics_UserValue=|TRAN_FourierNumHarmonics=10|TRAN_ShowMeasTableChart=False|TempSweep_Start_UserValue=20|TempSweep_Start=20|TempSweep_Stop_UserValue=26.85|TempSweep_Stop=26.85|TempSweep_Step_UserValue=5|TempSweep_Step=5|ParamSweep_Parameter1=R_ref|ParamSweep_Type1=LIST|ParamSweep_Start1=750.0k|ParamSweep_Stop1=2.250M|ParamSweep_Step1=1.6905Meg|ParamSweep_SweepType1=False|ParamSweep_SecondaryEnabled=True|ParamSweep_Parameter2=U_var|ParamSweep_Type2=LIST|ParamSweep_Start2=0|ParamSweep_Stop2=1.000|ParamSweep_Step2=1 2|ParamSweep_SweepType2=False|MonteCarlo_NumberOfRuns=10|MonteCarlo_DistributionType=GAUSS|MonteCarlo_Seed=-1|MonteCarlo_ResistorTolerance=10%|MonteCarlo_ResistorTolerance_UserValue=10%|MonteCarlo_CapacitorTolerance=10%|MonteCarlo_CapacitorTolerance_UserValue=10%|MonteCarlo_InductorTolerance=10%|MonteCarlo_InductorTolerance_UserValue=10%|MonteCarlo_TransistorTolerance=10%|MonteCarlo_TransistorTolerance_UserValue=10%|MonteCarlo_DCSourceTolerance=10%|MonteCarlo_DCSourceTolerance_UserValue=10%|MonteCarlo_DigitalTpTolerance=10%|MonteCarlo_DigitalTpTolerance_UserValue=10%|Sensitivity_Analysis=False|Sensitivity_GroupDeviationsEnabled=False|Sensitivity_GroupResistorEnabled=True|Sensitivity_GroupResistorDeviation_UserValue=|Sensitivity_GroupResistorDeviation=1m|Sensitivity_GroupCapacitorEnabled=False|Sensitivity_GroupCapacitorDeviation_UserValue=|Sensitivity_GroupCapacitorDeviation=1m|Sensitivity_GroupInductorEnabled=False|Sensitivity_GroupInductorDeviation_UserValue=|Sensitivity_GroupInductorDeviation=1m|Sensitivity_GroupTransistorEnabled=False|Sensitivity_GroupTransistorDeviation_UserValue=|Sensitivity_GroupTransistorDeviation=1m|Sensitivity_GroupDcSourceEnabled=False|Sensitivity_GroupDcSourceDeviation_UserValue=|Sensitivity_GroupDcSourceDeviation=1m|Sensitivity_GroupGlobalParameterEnabled=False|Sensitivity_GroupGlobalParameterDeviation_UserValue=|Sensitivity_GroupGlobalParameterDeviation=1m|Sensitivity_CustomDeviationsEnabled=True|OldCfgLoaded=True|SimViewSetup=ShowActiveSignalsProbes|OPTION_Method=Gear 2|OPTION_SpiceRefNode_UserValue=|OPTION_SpiceRefNode=GND|OPTION_DVCC_UserValue=|OPTION_DVCC=5|OPTION_DVDD_UserValue=|OPTION_DVDD=15|SheetsToNetlist=0|ParamSweep_CustomStart0_UserValue=1|ParamSweep_CustomStop0_UserValue=5|ParamSweep_CustomStart1_UserValue=|ParamSweep_CustomStop1_UserValue=|ParamSweep_CustomStart2_UserValue=|ParamSweep_CustomStop2_UserValue=|ParamSweep_Start1_UserValue=|ParamSweep_Stop1_UserValue=|ParamSweep_Start2_UserValue=|ParamSweep_Stop2_UserValue=|Sensitivity_ParameterDeviation0_UserValue=|OPTION_ITL4=100|LaunchDate=2025-09-18 09:37:42Z|DC_CustomStart0_UserValue=|DC_CustomStop0_UserValue=|DC_CustomStep0_UserValue=|DC_PrimaryStart_UserValue=|DC_PrimaryStop_UserValue=|DC_PrimaryStep_UserValue=|DC_CustomEnabled0=True|DC_CustomSource0=IC1A|DC_CustomStart0=1n|DC_CustomStop0=1u|DC_CustomStep0=100n|AC_VariableEnabled0=True|AC_XVariable0=|AC_Variable0=MAG(v(U_TRI))|AC_VariableName0=|AC_VariableUnits0=|AC_VariablePlot0=0|AC_VariableAxis0=0|AC_VariableColor0=8421504|TRAN_VariableEnabled0=True|TRAN_XVariable0=|TRAN_Variable0=v(U_SQR)|TRAN_VariableName0=U_SQR|TRAN_VariableUnits0=V|TRAN_VariablePlot0=1|TRAN_VariableAxis0=0|TRAN_VariableColor0=8421504|TRAN_VariableEnabled1=True|TRAN_XVariable1=|TRAN_Variable1=v(U_TRI)|TRAN_VariableName1=U_TRI|TRAN_VariableUnits1=V|TRAN_VariablePlot1=0|TRAN_VariableAxis1=0|TRAN_VariableColor1=8421504|TRAN_VariableEnabled2=True|TRAN_XVariable2=|TRAN_Variable2=v(U_SAW)|TRAN_VariableName2=U_SAW|TRAN_VariableUnits2=V|TRAN_VariablePlot2=2|TRAN_VariableAxis2=0|TRAN_VariableColor2=8421504|TRAN_VariableEnabled3=False|TRAN_XVariable3=|TRAN_Variable3=v(R_lambda_T)|TRAN_VariableName3=U_lambda_T|TRAN_VariableUnits3=V|TRAN_VariablePlot3=3|TRAN_VariableAxis3=0|TRAN_VariableColor3=8421504|TRAN_VariableEnabled4=False|TRAN_XVariable4=|TRAN_Variable4=v(U_C)|TRAN_VariableName4=U_C|TRAN_VariableUnits4=V|TRAN_VariablePlot4=3|TRAN_VariableAxis4=0|TRAN_VariableColor4=8421504|TRAN_VariableEnabled5=True|TRAN_XVariable5=|TRAN_Variable5=i(U_pos)*30|TRAN_VariableName5=P_Ges|TRAN_VariableUnits5=W|TRAN_VariablePlot5=3|TRAN_VariableAxis5=0|TRAN_VariableColor5=8421504|Variable0=v(U_SQR)|VariablePlot0=1|VariableAxis0=0|VariableName0=U_SQR|VariableUnits0=V|VariableColor0=8421504|Variable1=v(U_TRI)|VariablePlot1=0|VariableAxis1=0|VariableName1=U_TRI|VariableUnits1=V|VariableColor1=8421504|Variable2=v(U_SAW)|VariablePlot2=2|VariableAxis2=0|VariableName2=U_SAW|VariableUnits2=V|VariableColor2=8421504|Variable3=i(U_pos)*30|VariablePlot3=3|VariableAxis3=0|VariableName3=P_Ges|VariableUnits3=W|VariableColor3=8421504|ParamSweep_CustomEnabled0=False|ParamSweep_CustomParameter0=U_var|ParamSweep_CustomType0=LIST|ParamSweep_CustomStart0=1|ParamSweep_CustomStop0=5|ParamSweep_CustomStep0=1 1.083 1.166 1.25 1.333 1.416 1.5 1.583 1.666 1.75 1.833 1.916|ParamSweep_CustomEnabled1=True|ParamSweep_CustomParameter1=R_ref|ParamSweep_CustomType1=LIST|ParamSweep_CustomStart1=750.0k|ParamSweep_CustomStop1=2.250M|ParamSweep_CustomStep1=1.6905Meg|ParamSweep_CustomEnabled2=True|ParamSweep_CustomParameter2=U_var|ParamSweep_CustomType2=LIST|ParamSweep_CustomStart2=0|ParamSweep_CustomStop2=1.000|ParamSweep_CustomStep2=1 2|Sensitivity_ParameterEnabled0=True|Sensitivity_Parameter0=Temp|Sensitivity_ParameterDeviation0=1m</Config>
      <Results>
        <ResultConfig>
          <Name>Operating Point</Name>
          <Description />
          <Type>Operating Point</Type>
          <Date>2025-09-16 14:32:06Z</Date>
          <IsLocked>false</IsLocked>
          <Config>OP_Analysis=True|TRAN_Analysis=False|DC_Analysis=False|AC_Analysis=False|TF_Analysis=False|PZ_Analysis=False|Noise_Analysis=False|TRAN_FourierAnalysis=False|TempSweep_Analysis=False|ParamSweep_Analysis=True|MonteCarlo_Analysis=False|TF_Enabled=False|TF_Source=|TF_Reference=0|PZ_Enabled=False|PZ_Node1=|PZ_Node2=0|PZ_Node3=|PZ_Node4=0|PZ_AnalType=PZ|PZ_TfType=VOL|AnalysesDataSavedIndex=2|DC_ShowMeasTableChart=False|DC_PrimarySource=IC1A|DC_PrimaryStart=1n|DC_PrimaryStop=1u|DC_PrimaryStep=100n|DC_EnableSecondary=False|DC_SecondarySource=|DC_SecondaryStart=|DC_SecondaryStop=|DC_SecondaryStep=|Noise_Enabled=False|Noise_Source=|Noise_Output=|Noise_Reference=0|Noise_Start_UserValue=20|Noise_Start=20|Noise_Stop_UserValue=20k|Noise_Stop=20k|Noise_TestPoints_UserValue=10|Noise_TestPoints=10|Noise_PointsPerSummary=0|Noise_SweepType=DEC|AC_StartFrequency_UserValue=20|AC_StartFrequency=20|AC_StopFrequency_UserValue=20k|AC_StopFrequency=20k|AC_TestPoints_UserValue=10|AC_TestPoints=10|AC_SweepType=DEC|AC_ShowMeasTableChart=False|TRAN_StartTime_UserValue=10m|TRAN_StartTime=10m|TRAN_StopTime_UserValue=16m|TRAN_StopTime=16m|TRAN_StepTime_UserValue=1u|TRAN_StepTime=1u|TRAN_MaxStepTime_UserValue=1u|TRAN_MaxStepTime=1u|TRAN_AlwaysSetDefaults=False|TRAN_DefaultCycles_UserValue=5|TRAN_DefaultCycles=5|TRAN_DefaultPointsPerCycle_UserValue=50|TRAN_DefaultPointsPerCycle=50|TRAN_UseInitialConditions=True|TRAN_FourierEnabled=False|TRAN_FourierFundFreq_UserValue=|TRAN_FourierFundFreq=1Meg|TRAN_FourierNumHarmonics_UserValue=|TRAN_FourierNumHarmonics=10|TRAN_ShowMeasTableChart=False|TempSweep_Start_UserValue=20|TempSweep_Start=20|TempSweep_Stop_UserValue=26.85|TempSweep_Stop=26.85|TempSweep_Step_UserValue=5|TempSweep_Step=5|ParamSweep_Parameter1=R_ref|ParamSweep_Type1=LIST|ParamSweep_Start1=750.0k|ParamSweep_Stop1=2.250M|ParamSweep_Step1=1.6905Meg|ParamSweep_SweepType1=False|ParamSweep_SecondaryEnabled=True|ParamSweep_Parameter2=U_var|ParamSweep_Type2=LIST|ParamSweep_Start2=0|ParamSweep_Stop2=1.000|ParamSweep_Step2=1.08333|ParamSweep_SweepType2=False|MonteCarlo_NumberOfRuns=10|MonteCarlo_DistributionType=GAUSS|MonteCarlo_Seed=-1|MonteCarlo_ResistorTolerance=10%|MonteCarlo_ResistorTolerance_UserValue=10%|MonteCarlo_CapacitorTolerance=10%|MonteCarlo_CapacitorTolerance_UserValue=10%|MonteCarlo_InductorTolerance=10%|MonteCarlo_InductorTolerance_UserValue=10%|MonteCarlo_TransistorTolerance=10%|MonteCarlo_TransistorTolerance_UserValue=10%|MonteCarlo_DCSourceTolerance=10%|MonteCarlo_DCSourceTolerance_UserValue=10%|MonteCarlo_DigitalTpTolerance=10%|MonteCarlo_DigitalTpTolerance_UserValue=10%|Sensitivity_Analysis=False|Sensitivity_GroupDeviationsEnabled=False|Sensitivity_GroupResistorEnabled=True|Sensitivity_GroupResistorDeviation_UserValue=|Sensitivity_GroupResistorDeviation=1m|Sensitivity_GroupCapacitorEnabled=False|Sensitivity_GroupCapacitorDeviation_UserValue=|Sensitivity_GroupCapacitorDeviation=1m|Sensitivity_GroupInductorEnabled=False|Sensitivity_GroupInductorDeviation_UserValue=|Sensitivity_GroupInductorDeviation=1m|Sensitivity_GroupTransistorEnabled=False|Sensitivity_GroupTransistorDeviation_UserValue=|Sensitivity_GroupTransistorDeviation=1m|Sensitivity_GroupDcSourceEnabled=False|Sensitivity_GroupDcSourceDeviation_UserValue=|Sensitivity_GroupDcSourceDeviation=1m|Sensitivity_GroupGlobalParameterEnabled=False|Sensitivity_GroupGlobalParameterDeviation_UserValue=|Sensitivity_GroupGlobalParameterDeviation=1m|Sensitivity_CustomDeviationsEnabled=True|OldCfgLoaded=True|SimViewSetup=ShowActiveSignalsProbes|OPTION_Method=Gear 2|OPTION_SpiceRefNode_UserValue=|OPTION_SpiceRefNode=GND|OPTION_DVCC_UserValue=|OPTION_DVCC=5|OPTION_DVDD_UserValue=|OPTION_DVDD=15|SheetsToNetlist=0|ParamSweep_CustomStart0_UserValue=1|ParamSweep_CustomStop0_UserValue=5|ParamSweep_CustomStep0_UserValue=2|ParamSweep_Start1_UserValue=|ParamSweep_Stop1_UserValue=|ParamSweep_Step1_UserValue=2|Sensitivity_ParameterDeviation0_UserValue=|LaunchDate=2025-09-16 14:32:06Z|DC_CustomStart0_UserValue=|DC_CustomStop0_UserValue=|DC_CustomStep0_UserValue=|DC_PrimaryStart_UserValue=|DC_PrimaryStop_UserValue=|DC_PrimaryStep_UserValue=|ParamSweep_CustomStart1_UserValue=|ParamSweep_CustomStop1_UserValue=|ParamSweep_CustomStep1_UserValue=100pF|ParamSweep_Start2_UserValue=|ParamSweep_Stop2_UserValue=|OPTION_ITL4=100|ParamSweep_CustomStart2_UserValue=|ParamSweep_CustomStop2_UserValue=|DC_CustomEnabled0=True|DC_CustomSource0=IC1A|DC_CustomStart0=1n|DC_CustomStop0=1u|DC_CustomStep0=100n|AC_VariableEnabled0=True|AC_XVariable0=|AC_Variable0=MAG(v(U_TRI))|AC_VariableName0=|AC_VariableUnits0=|AC_VariablePlot0=0|AC_VariableAxis0=0|AC_VariableColor0=8421504|TRAN_VariableEnabled0=True|TRAN_XVariable0=|TRAN_Variable0=v(U_SQR)|TRAN_VariableName0=U_SQR|TRAN_VariableUnits0=V|TRAN_VariablePlot0=1|TRAN_VariableAxis0=0|TRAN_VariableColor0=8421504|TRAN_VariableEnabled1=True|TRAN_XVariable1=|TRAN_Variable1=v(U_TRI)|TRAN_VariableName1=U_TRI|TRAN_VariableUnits1=V|TRAN_VariablePlot1=0|TRAN_VariableAxis1=0|TRAN_VariableColor1=8421504|TRAN_VariableEnabled2=True|TRAN_XVariable2=|TRAN_Variable2=v(U_SQR_OTA)-v(U_TRI)|TRAN_VariableName2=Delta-V @ OTA-B|TRAN_VariableUnits2=V|TRAN_VariablePlot2=2|TRAN_VariableAxis2=0|TRAN_VariableColor2=8421504|TRAN_VariableEnabled3=True|TRAN_XVariable3=|TRAN_Variable3=v(R_lambda_T)|TRAN_VariableName3=U_lambda_T|TRAN_VariableUnits3=V|TRAN_VariablePlot3=3|TRAN_VariableAxis3=0|TRAN_VariableColor3=8421504|TRAN_VariableEnabled4=True|TRAN_XVariable4=|TRAN_Variable4=i(U_mess)|TRAN_VariableName4=I_ABC|TRAN_VariableUnits4=A|TRAN_VariablePlot4=4|TRAN_VariableAxis4=0|TRAN_VariableColor4=8421504|TRAN_VariableEnabled5=True|TRAN_XVariable5=|TRAN_Variable5=v(U_C)|TRAN_VariableName5=U_C|TRAN_VariableUnits5=V|TRAN_VariablePlot5=3|TRAN_VariableAxis5=0|TRAN_VariableColor5=8421504|TRAN_VariableEnabled6=True|TRAN_XVariable6=|TRAN_Variable6=i(U_messref)|TRAN_VariableName6=I_ref + I_ABC|TRAN_VariableUnits6=A|TRAN_VariablePlot6=4|TRAN_VariableAxis6=0|TRAN_VariableColor6=8421504|TRAN_VariableEnabled7=True|TRAN_XVariable7=|TRAN_Variable7=v(U_SAW)|TRAN_VariableName7=U_SAW|TRAN_VariableUnits7=V|TRAN_VariablePlot7=5|TRAN_VariableAxis7=0|TRAN_VariableColor7=8421504|ParamSweep_CustomEnabled0=False|ParamSweep_CustomParameter0=U_var|ParamSweep_CustomType0=LIST|ParamSweep_CustomStart0=1|ParamSweep_CustomStop0=5|ParamSweep_CustomStep0=1 1.083 1.166 1.25 1.333 1.416 1.5 1.583 1.666 1.75 1.833 1.916|ParamSweep_CustomEnabled1=True|ParamSweep_CustomParameter1=R_ref|ParamSweep_CustomType1=LIST|ParamSweep_CustomStart1=750.0k|ParamSweep_CustomStop1=2.250M|ParamSweep_CustomStep1=1.6905Meg|ParamSweep_CustomEnabled2=True|ParamSweep_CustomParameter2=U_var|ParamSweep_CustomType2=LIST|ParamSweep_CustomStart2=0|ParamSweep_CustomStop2=1.000|ParamSweep_CustomStep2=1.08333|Sensitivity_ParameterEnabled0=True|Sensitivity_Parameter0=Temp|Sensitivity_ParameterDeviation0=1m</Config>
          <Charts>
            <ChartConfig>
              <Name>Operating Point</Name>
              <Id>VAFWHAPQ</Id>
            </ChartConfig>
          </Charts>
        </ResultConfig>
        <ResultConfig>
          <Name>DC Sweep</Name>
          <Description />
          <Type>DC Sweep</Type>
          <Date>2025-09-16 14:32:08Z</Date>
          <IsLocked>false</IsLocked>
          <Config>OP_Analysis=False|TRAN_Analysis=False|DC_Analysis=True|AC_Analysis=False|TF_Analysis=False|PZ_Analysis=False|Noise_Analysis=False|TRAN_FourierAnalysis=False|TempSweep_Analysis=False|ParamSweep_Analysis=True|MonteCarlo_Analysis=False|TF_Enabled=False|TF_Source=|TF_Reference=0|PZ_Enabled=False|PZ_Node1=|PZ_Node2=0|PZ_Node3=|PZ_Node4=0|PZ_AnalType=PZ|PZ_TfType=VOL|AnalysesDataSavedIndex=4|DC_ShowMeasTableChart=False|DC_PrimarySource=IC1A|DC_PrimaryStart=1n|DC_PrimaryStop=1u|DC_PrimaryStep=100n|DC_EnableSecondary=False|DC_SecondarySource=|DC_SecondaryStart=|DC_SecondaryStop=|DC_SecondaryStep=|Noise_Enabled=False|Noise_Source=|Noise_Output=|Noise_Reference=0|Noise_Start_UserValue=20|Noise_Start=20|Noise_Stop_UserValue=20k|Noise_Stop=20k|Noise_TestPoints_UserValue=10|Noise_TestPoints=10|Noise_PointsPerSummary=0|Noise_SweepType=DEC|AC_StartFrequency_UserValue=20|AC_StartFrequency=20|AC_StopFrequency_UserValue=20k|AC_StopFrequency=20k|AC_TestPoints_UserValue=10|AC_TestPoints=10|AC_SweepType=DEC|AC_ShowMeasTableChart=False|TRAN_StartTime_UserValue=10m|TRAN_StartTime=10m|TRAN_StopTime_UserValue=16m|TRAN_StopTime=16m|TRAN_StepTime_UserValue=1u|TRAN_StepTime=1u|TRAN_MaxStepTime_UserValue=1u|TRAN_MaxStepTime=1u|TRAN_AlwaysSetDefaults=False|TRAN_DefaultCycles_UserValue=5|TRAN_DefaultCycles=5|TRAN_DefaultPointsPerCycle_UserValue=50|TRAN_DefaultPointsPerCycle=50|TRAN_UseInitialConditions=True|TRAN_FourierEnabled=False|TRAN_FourierFundFreq_UserValue=|TRAN_FourierFundFreq=1Meg|TRAN_FourierNumHarmonics_UserValue=|TRAN_FourierNumHarmonics=10|TRAN_ShowMeasTableChart=False|TempSweep_Start_UserValue=20|TempSweep_Start=20|TempSweep_Stop_UserValue=26.85|TempSweep_Stop=26.85|TempSweep_Step_UserValue=5|TempSweep_Step=5|ParamSweep_Parameter1=R_ref|ParamSweep_Type1=LIST|ParamSweep_Start1=|ParamSweep_Stop1=|ParamSweep_Step1=1.6905Meg|ParamSweep_SweepType1=False|ParamSweep_SecondaryEnabled=True|ParamSweep_Parameter2=U_var|ParamSweep_Type2=LIST|ParamSweep_Start2=|ParamSweep_Stop2=|ParamSweep_Step2=1.08333|ParamSweep_SweepType2=False|MonteCarlo_NumberOfRuns=10|MonteCarlo_DistributionType=GAUSS|MonteCarlo_Seed=-1|MonteCarlo_ResistorTolerance=10%|MonteCarlo_ResistorTolerance_UserValue=10%|MonteCarlo_CapacitorTolerance=10%|MonteCarlo_CapacitorTolerance_UserValue=10%|MonteCarlo_InductorTolerance=10%|MonteCarlo_InductorTolerance_UserValue=10%|MonteCarlo_TransistorTolerance=10%|MonteCarlo_TransistorTolerance_UserValue=10%|MonteCarlo_DCSourceTolerance=10%|MonteCarlo_DCSourceTolerance_UserValue=10%|MonteCarlo_DigitalTpTolerance=10%|MonteCarlo_DigitalTpTolerance_UserValue=10%|Sensitivity_Analysis=False|Sensitivity_GroupDeviationsEnabled=False|Sensitivity_GroupResistorEnabled=True|Sensitivity_GroupResistorDeviation_UserValue=|Sensitivity_GroupResistorDeviation=1m|Sensitivity_GroupCapacitorEnabled=False|Sensitivity_GroupCapacitorDeviation_UserValue=|Sensitivity_GroupCapacitorDeviation=1m|Sensitivity_GroupInductorEnabled=False|Sensitivity_GroupInductorDeviation_UserValue=|Sensitivity_GroupInductorDeviation=1m|Sensitivity_GroupTransistorEnabled=False|Sensitivity_GroupTransistorDeviation_UserValue=|Sensitivity_GroupTransistorDeviation=1m|Sensitivity_GroupDcSourceEnabled=False|Sensitivity_GroupDcSourceDeviation_UserValue=|Sensitivity_GroupDcSourceDeviation=1m|Sensitivity_GroupGlobalParameterEnabled=False|Sensitivity_GroupGlobalParameterDeviation_UserValue=|Sensitivity_GroupGlobalParameterDeviation=1m|Sensitivity_CustomDeviationsEnabled=True|OldCfgLoaded=True|SimViewSetup=ShowActiveSignalsProbes|OPTION_Method=Gear 2|OPTION_SpiceRefNode_UserValue=|OPTION_SpiceRefNode=GND|OPTION_DVCC_UserValue=|OPTION_DVCC=5|OPTION_DVDD_UserValue=|OPTION_DVDD=15|SheetsToNetlist=0|ParamSweep_CustomStart0_UserValue=1|ParamSweep_CustomStop0_UserValue=5|ParamSweep_CustomStep0_UserValue=2|ParamSweep_Start1_UserValue=|ParamSweep_Stop1_UserValue=|ParamSweep_Step1_UserValue=2|Sensitivity_ParameterDeviation0_UserValue=|LaunchDate=2025-09-16 14:32:08Z|DC_CustomStart0_UserValue=|DC_CustomStop0_UserValue=|DC_CustomStep0_UserValue=|DC_PrimaryStart_UserValue=|DC_PrimaryStop_UserValue=|DC_PrimaryStep_UserValue=|ParamSweep_CustomStart1_UserValue=|ParamSweep_CustomStop1_UserValue=|ParamSweep_CustomStep1_UserValue=100pF|ParamSweep_Start2_UserValue=|ParamSweep_Stop2_UserValue=|OPTION_ITL4=100|ParamSweep_CustomStart2_UserValue=|ParamSweep_CustomStop2_UserValue=|AC_VariableEnabled0=True|AC_XVariable0=|AC_Variable0=MAG(v(U_TRI))|AC_VariableName0=|AC_VariableUnits0=|AC_VariablePlot0=0|AC_VariableAxis0=0|AC_VariableColor0=8421504|TRAN_VariableEnabled0=True|TRAN_XVariable0=|TRAN_Variable0=v(U_SQR)|TRAN_VariableName0=U_SQR|TRAN_VariableUnits0=V|TRAN_VariablePlot0=1|TRAN_VariableAxis0=0|TRAN_VariableColor0=8421504|TRAN_VariableEnabled1=True|TRAN_XVariable1=|TRAN_Variable1=v(U_TRI)|TRAN_VariableName1=U_TRI|TRAN_VariableUnits1=V|TRAN_VariablePlot1=0|TRAN_VariableAxis1=0|TRAN_VariableColor1=8421504|TRAN_VariableEnabled2=True|TRAN_XVariable2=|TRAN_Variable2=v(U_SQR_OTA)-v(U_TRI)|TRAN_VariableName2=Delta-V @ OTA-B|TRAN_VariableUnits2=V|TRAN_VariablePlot2=2|TRAN_VariableAxis2=0|TRAN_VariableColor2=8421504|TRAN_VariableEnabled3=True|TRAN_XVariable3=|TRAN_Variable3=v(R_lambda_T)|TRAN_VariableName3=U_lambda_T|TRAN_VariableUnits3=V|TRAN_VariablePlot3=3|TRAN_VariableAxis3=0|TRAN_VariableColor3=8421504|TRAN_VariableEnabled4=True|TRAN_XVariable4=|TRAN_Variable4=i(U_mess)|TRAN_VariableName4=I_ABC|TRAN_VariableUnits4=A|TRAN_VariablePlot4=4|TRAN_VariableAxis4=0|TRAN_VariableColor4=8421504|TRAN_VariableEnabled5=True|TRAN_XVariable5=|TRAN_Variable5=v(U_C)|TRAN_VariableName5=U_C|TRAN_VariableUnits5=V|TRAN_VariablePlot5=3|TRAN_VariableAxis5=0|TRAN_VariableColor5=8421504|TRAN_VariableEnabled6=True|TRAN_XVariable6=|TRAN_Variable6=i(U_messref)|TRAN_VariableName6=I_ref + I_ABC|TRAN_VariableUnits6=A|TRAN_VariablePlot6=4|TRAN_VariableAxis6=0|TRAN_VariableColor6=8421504|TRAN_VariableEnabled7=True|TRAN_XVariable7=|TRAN_Variable7=v(U_SAW)|TRAN_VariableName7=U_SAW|TRAN_VariableUnits7=V|TRAN_VariablePlot7=5|TRAN_VariableAxis7=0|TRAN_VariableColor7=8421504|DC_CustomEnabled0=True|DC_CustomSource0=IC1A|DC_CustomStart0=1n|DC_CustomStop0=1u|DC_CustomStep0=100n|ParamSweep_CustomEnabled0=False|ParamSweep_CustomParameter0=U_var|ParamSweep_CustomType0=LIST|ParamSweep_CustomStart0=1|ParamSweep_CustomStop0=5|ParamSweep_CustomStep0=1 1.083 1.166 1.25 1.333 1.416 1.5 1.583 1.666 1.75 1.833 1.916|ParamSweep_CustomEnabled1=True|ParamSweep_CustomParameter1=R_ref|ParamSweep_CustomType1=LIST|ParamSweep_CustomStart1=|ParamSweep_CustomStop1=|ParamSweep_CustomStep1=1.6905Meg|ParamSweep_CustomEnabled2=True|ParamSweep_CustomParameter2=U_var|ParamSweep_CustomType2=LIST|ParamSweep_CustomStart2=|ParamSweep_CustomStop2=|ParamSweep_CustomStep2=1.08333|Sensitivity_ParameterEnabled0=True|Sensitivity_Parameter0=Temp|Sensitivity_ParameterDeviation0=1m</Config>
          <Charts />
        </ResultConfig>
        <ResultConfig>
          <Name>Transient Analysis</Name>
          <Description />
          <Type>Transient Analysis</Type>
          <Date>2025-09-18 09:37:42Z</Date>
          <IsLocked>false</IsLocked>
          <Config>OP_Analysis=False|TRAN_Analysis=True|DC_Analysis=False|AC_Analysis=False|TF_Analysis=False|PZ_Analysis=False|Noise_Analysis=False|TRAN_FourierAnalysis=False|TempSweep_Analysis=False|ParamSweep_Analysis=False|MonteCarlo_Analysis=False|TF_Enabled=False|TF_Source=|TF_Reference=0|PZ_Enabled=False|PZ_Node1=|PZ_Node2=0|PZ_Node3=|PZ_Node4=0|PZ_AnalType=PZ|PZ_TfType=VOL|AnalysesDataSavedIndex=4|DC_ShowMeasTableChart=False|DC_PrimarySource=IC1A|DC_PrimaryStart=1n|DC_PrimaryStop=1u|DC_PrimaryStep=100n|DC_EnableSecondary=False|DC_SecondarySource=|DC_SecondaryStart=|DC_SecondaryStop=|DC_SecondaryStep=|Noise_Enabled=False|Noise_Source=|Noise_Output=|Noise_Reference=0|Noise_Start_UserValue=20|Noise_Start=20|Noise_Stop_UserValue=20k|Noise_Stop=20k|Noise_TestPoints_UserValue=10|Noise_TestPoints=10|Noise_PointsPerSummary=0|Noise_SweepType=DEC|AC_StartFrequency_UserValue=20|AC_StartFrequency=20|AC_StopFrequency_UserValue=20k|AC_StopFrequency=20k|AC_TestPoints_UserValue=10|AC_TestPoints=10|AC_SweepType=DEC|AC_ShowMeasTableChart=False|TRAN_StartTime_UserValue=10m|TRAN_StartTime=10m|TRAN_StopTime_UserValue=16m|TRAN_StopTime=16m|TRAN_StepTime_UserValue=1u|TRAN_StepTime=1u|TRAN_MaxStepTime_UserValue=1u|TRAN_MaxStepTime=1u|TRAN_AlwaysSetDefaults=False|TRAN_DefaultCycles_UserValue=5|TRAN_DefaultCycles=5|TRAN_DefaultPointsPerCycle_UserValue=50|TRAN_DefaultPointsPerCycle=50|TRAN_UseInitialConditions=False|TRAN_FourierEnabled=False|TRAN_FourierFundFreq_UserValue=|TRAN_FourierFundFreq=1Meg|TRAN_FourierNumHarmonics_UserValue=|TRAN_FourierNumHarmonics=10|TRAN_ShowMeasTableChart=False|TempSweep_Start_UserValue=20|TempSweep_Start=20|TempSweep_Stop_UserValue=26.85|TempSweep_Stop=26.85|TempSweep_Step_UserValue=5|TempSweep_Step=5|ParamSweep_Parameter1=R_ref|ParamSweep_Type1=LIST|ParamSweep_Start1=750.0k|ParamSweep_Stop1=2.250M|ParamSweep_Step1=1.6905Meg|ParamSweep_SweepType1=False|ParamSweep_SecondaryEnabled=True|ParamSweep_Parameter2=U_var|ParamSweep_Type2=LIST|ParamSweep_Start2=0|ParamSweep_Stop2=1.000|ParamSweep_Step2=1 2|ParamSweep_SweepType2=False|MonteCarlo_NumberOfRuns=10|MonteCarlo_DistributionType=GAUSS|MonteCarlo_Seed=-1|MonteCarlo_ResistorTolerance=10%|MonteCarlo_ResistorTolerance_UserValue=10%|MonteCarlo_CapacitorTolerance=10%|MonteCarlo_CapacitorTolerance_UserValue=10%|MonteCarlo_InductorTolerance=10%|MonteCarlo_InductorTolerance_UserValue=10%|MonteCarlo_TransistorTolerance=10%|MonteCarlo_TransistorTolerance_UserValue=10%|MonteCarlo_DCSourceTolerance=10%|MonteCarlo_DCSourceTolerance_UserValue=10%|MonteCarlo_DigitalTpTolerance=10%|MonteCarlo_DigitalTpTolerance_UserValue=10%|Sensitivity_Analysis=False|Sensitivity_GroupDeviationsEnabled=False|Sensitivity_GroupResistorEnabled=True|Sensitivity_GroupResistorDeviation_UserValue=|Sensitivity_GroupResistorDeviation=1m|Sensitivity_GroupCapacitorEnabled=False|Sensitivity_GroupCapacitorDeviation_UserValue=|Sensitivity_GroupCapacitorDeviation=1m|Sensitivity_GroupInductorEnabled=False|Sensitivity_GroupInductorDeviation_UserValue=|Sensitivity_GroupInductorDeviation=1m|Sensitivity_GroupTransistorEnabled=False|Sensitivity_GroupTransistorDeviation_UserValue=|Sensitivity_GroupTransistorDeviation=1m|Sensitivity_GroupDcSourceEnabled=False|Sensitivity_GroupDcSourceDeviation_UserValue=|Sensitivity_GroupDcSourceDeviation=1m|Sensitivity_GroupGlobalParameterEnabled=False|Sensitivity_GroupGlobalParameterDeviation_UserValue=|Sensitivity_GroupGlobalParameterDeviation=1m|Sensitivity_CustomDeviationsEnabled=True|OldCfgLoaded=True|SimViewSetup=ShowActiveSignalsProbes|OPTION_Method=Gear 2|OPTION_SpiceRefNode_UserValue=|OPTION_SpiceRefNode=GND|OPTION_DVCC_UserValue=|OPTION_DVCC=5|OPTION_DVDD_UserValue=|OPTION_DVDD=15|SheetsToNetlist=0|ParamSweep_CustomStart0_UserValue=1|ParamSweep_CustomStop0_UserValue=5|ParamSweep_CustomStart1_UserValue=|ParamSweep_CustomStop1_UserValue=|ParamSweep_CustomStart2_UserValue=|ParamSweep_CustomStop2_UserValue=|ParamSweep_Start1_UserValue=|ParamSweep_Stop1_UserValue=|ParamSweep_Start2_UserValue=|ParamSweep_Stop2_UserValue=|Sensitivity_ParameterDeviation0_UserValue=|OPTION_ITL4=100|LaunchDate=2025-09-18 09:37:42Z|DC_CustomStart0_UserValue=|DC_CustomStop0_UserValue=|DC_CustomStep0_UserValue=|DC_PrimaryStart_UserValue=|DC_PrimaryStop_UserValue=|DC_PrimaryStep_UserValue=|DC_CustomEnabled0=True|DC_CustomSource0=IC1A|DC_CustomStart0=1n|DC_CustomStop0=1u|DC_CustomStep0=100n|AC_VariableEnabled0=True|AC_XVariable0=|AC_Variable0=MAG(v(U_TRI))|AC_VariableName0=|AC_VariableUnits0=|AC_VariablePlot0=0|AC_VariableAxis0=0|AC_VariableColor0=8421504|TRAN_VariableEnabled0=True|TRAN_XVariable0=|TRAN_Variable0=v(U_SQR)|TRAN_VariableName0=U_SQR|TRAN_VariableUnits0=V|TRAN_VariablePlot0=1|TRAN_VariableAxis0=0|TRAN_VariableColor0=8421504|TRAN_VariableEnabled1=True|TRAN_XVariable1=|TRAN_Variable1=v(U_TRI)|TRAN_VariableName1=U_TRI|TRAN_VariableUnits1=V|TRAN_VariablePlot1=0|TRAN_VariableAxis1=0|TRAN_VariableColor1=8421504|TRAN_VariableEnabled2=True|TRAN_XVariable2=|TRAN_Variable2=v(U_SAW)|TRAN_VariableName2=U_SAW|TRAN_VariableUnits2=V|TRAN_VariablePlot2=2|TRAN_VariableAxis2=0|TRAN_VariableColor2=8421504|TRAN_VariableEnabled3=False|TRAN_XVariable3=|TRAN_Variable3=v(R_lambda_T)|TRAN_VariableName3=U_lambda_T|TRAN_VariableUnits3=V|TRAN_VariablePlot3=3|TRAN_VariableAxis3=0|TRAN_VariableColor3=8421504|TRAN_VariableEnabled4=False|TRAN_XVariable4=|TRAN_Variable4=v(U_C)|TRAN_VariableName4=U_C|TRAN_VariableUnits4=V|TRAN_VariablePlot4=3|TRAN_VariableAxis4=0|TRAN_VariableColor4=8421504|TRAN_VariableEnabled5=True|TRAN_XVariable5=|TRAN_Variable5=i(U_pos)*30|TRAN_VariableName5=P_Ges|TRAN_VariableUnits5=W|TRAN_VariablePlot5=3|TRAN_VariableAxis5=0|TRAN_VariableColor5=8421504|Variable0=v(U_SQR)|VariablePlot0=1|VariableAxis0=0|VariableName0=U_SQR|VariableUnits0=V|VariableColor0=8421504|Variable1=v(U_TRI)|VariablePlot1=0|VariableAxis1=0|VariableName1=U_TRI|VariableUnits1=V|VariableColor1=8421504|Variable2=v(U_SAW)|VariablePlot2=2|VariableAxis2=0|VariableName2=U_SAW|VariableUnits2=V|VariableColor2=8421504|Variable3=i(U_pos)*30|VariablePlot3=3|VariableAxis3=0|VariableName3=P_Ges|VariableUnits3=W|VariableColor3=8421504|ParamSweep_CustomEnabled0=False|ParamSweep_CustomParameter0=U_var|ParamSweep_CustomType0=LIST|ParamSweep_CustomStart0=1|ParamSweep_CustomStop0=5|ParamSweep_CustomStep0=1 1.083 1.166 1.25 1.333 1.416 1.5 1.583 1.666 1.75 1.833 1.916|ParamSweep_CustomEnabled1=True|ParamSweep_CustomParameter1=R_ref|ParamSweep_CustomType1=LIST|ParamSweep_CustomStart1=750.0k|ParamSweep_CustomStop1=2.250M|ParamSweep_CustomStep1=1.6905Meg|ParamSweep_CustomEnabled2=True|ParamSweep_CustomParameter2=U_var|ParamSweep_CustomType2=LIST|ParamSweep_CustomStart2=0|ParamSweep_CustomStop2=1.000|ParamSweep_CustomStep2=1 2|Sensitivity_ParameterEnabled0=True|Sensitivity_Parameter0=Temp|Sensitivity_ParameterDeviation0=1m</Config>
          <Charts>
            <ChartConfig>
              <Name>Transient Analysis</Name>
              <Id>NQKSUMXL</Id>
            </ChartConfig>
          </Charts>
        </ResultConfig>
        <ResultConfig>
          <Name>AC Analysis</Name>
          <Description />
          <Type>AC Analysis</Type>
          <Date>2025-09-16 14:32:12Z</Date>
          <IsLocked>false</IsLocked>
          <Config>OP_Analysis=False|TRAN_Analysis=False|DC_Analysis=False|AC_Analysis=True|TF_Analysis=False|PZ_Analysis=False|Noise_Analysis=False|TRAN_FourierAnalysis=False|TempSweep_Analysis=False|ParamSweep_Analysis=True|MonteCarlo_Analysis=False|TF_Enabled=False|TF_Source=|TF_Reference=0|PZ_Enabled=False|PZ_Node1=|PZ_Node2=0|PZ_Node3=|PZ_Node4=0|PZ_AnalType=PZ|PZ_TfType=VOL|AnalysesDataSavedIndex=4|DC_ShowMeasTableChart=False|DC_PrimarySource=IC1A|DC_PrimaryStart=1n|DC_PrimaryStop=1u|DC_PrimaryStep=100n|DC_EnableSecondary=False|DC_SecondarySource=|DC_SecondaryStart=|DC_SecondaryStop=|DC_SecondaryStep=|Noise_Enabled=False|Noise_Source=|Noise_Output=|Noise_Reference=0|Noise_Start_UserValue=20|Noise_Start=20|Noise_Stop_UserValue=20k|Noise_Stop=20k|Noise_TestPoints_UserValue=10|Noise_TestPoints=10|Noise_PointsPerSummary=0|Noise_SweepType=DEC|AC_StartFrequency_UserValue=20|AC_StartFrequency=20|AC_StopFrequency_UserValue=20k|AC_StopFrequency=20k|AC_TestPoints_UserValue=10|AC_TestPoints=10|AC_SweepType=DEC|AC_ShowMeasTableChart=False|TRAN_StartTime_UserValue=10m|TRAN_StartTime=10m|TRAN_StopTime_UserValue=16m|TRAN_StopTime=16m|TRAN_StepTime_UserValue=1u|TRAN_StepTime=1u|TRAN_MaxStepTime_UserValue=1u|TRAN_MaxStepTime=1u|TRAN_AlwaysSetDefaults=False|TRAN_DefaultCycles_UserValue=5|TRAN_DefaultCycles=5|TRAN_DefaultPointsPerCycle_UserValue=50|TRAN_DefaultPointsPerCycle=50|TRAN_UseInitialConditions=True|TRAN_FourierEnabled=False|TRAN_FourierFundFreq_UserValue=|TRAN_FourierFundFreq=1Meg|TRAN_FourierNumHarmonics_UserValue=|TRAN_FourierNumHarmonics=10|TRAN_ShowMeasTableChart=False|TempSweep_Start_UserValue=20|TempSweep_Start=20|TempSweep_Stop_UserValue=26.85|TempSweep_Stop=26.85|TempSweep_Step_UserValue=5|TempSweep_Step=5|ParamSweep_Parameter1=R_ref|ParamSweep_Type1=LIST|ParamSweep_Start1=|ParamSweep_Stop1=|ParamSweep_Step1=1.6905Meg|ParamSweep_SweepType1=False|ParamSweep_SecondaryEnabled=True|ParamSweep_Parameter2=U_var|ParamSweep_Type2=LIST|ParamSweep_Start2=|ParamSweep_Stop2=|ParamSweep_Step2=1.08333|ParamSweep_SweepType2=False|MonteCarlo_NumberOfRuns=10|MonteCarlo_DistributionType=GAUSS|MonteCarlo_Seed=-1|MonteCarlo_ResistorTolerance=10%|MonteCarlo_ResistorTolerance_UserValue=10%|MonteCarlo_CapacitorTolerance=10%|MonteCarlo_CapacitorTolerance_UserValue=10%|MonteCarlo_InductorTolerance=10%|MonteCarlo_InductorTolerance_UserValue=10%|MonteCarlo_TransistorTolerance=10%|MonteCarlo_TransistorTolerance_UserValue=10%|MonteCarlo_DCSourceTolerance=10%|MonteCarlo_DCSourceTolerance_UserValue=10%|MonteCarlo_DigitalTpTolerance=10%|MonteCarlo_DigitalTpTolerance_UserValue=10%|Sensitivity_Analysis=False|Sensitivity_GroupDeviationsEnabled=False|Sensitivity_GroupResistorEnabled=True|Sensitivity_GroupResistorDeviation_UserValue=|Sensitivity_GroupResistorDeviation=1m|Sensitivity_GroupCapacitorEnabled=False|Sensitivity_GroupCapacitorDeviation_UserValue=|Sensitivity_GroupCapacitorDeviation=1m|Sensitivity_GroupInductorEnabled=False|Sensitivity_GroupInductorDeviation_UserValue=|Sensitivity_GroupInductorDeviation=1m|Sensitivity_GroupTransistorEnabled=False|Sensitivity_GroupTransistorDeviation_UserValue=|Sensitivity_GroupTransistorDeviation=1m|Sensitivity_GroupDcSourceEnabled=False|Sensitivity_GroupDcSourceDeviation_UserValue=|Sensitivity_GroupDcSourceDeviation=1m|Sensitivity_GroupGlobalParameterEnabled=False|Sensitivity_GroupGlobalParameterDeviation_UserValue=|Sensitivity_GroupGlobalParameterDeviation=1m|Sensitivity_CustomDeviationsEnabled=True|OldCfgLoaded=True|SimViewSetup=ShowActiveSignalsProbes|OPTION_Method=Gear 2|OPTION_SpiceRefNode_UserValue=|OPTION_SpiceRefNode=GND|OPTION_DVCC_UserValue=|OPTION_DVCC=5|OPTION_DVDD_UserValue=|OPTION_DVDD=15|SheetsToNetlist=0|ParamSweep_CustomStart0_UserValue=1|ParamSweep_CustomStop0_UserValue=5|ParamSweep_CustomStep0_UserValue=2|ParamSweep_Start1_UserValue=|ParamSweep_Stop1_UserValue=|ParamSweep_Step1_UserValue=2|Sensitivity_ParameterDeviation0_UserValue=|LaunchDate=2025-09-16 14:32:12Z|DC_CustomStart0_UserValue=|DC_CustomStop0_UserValue=|DC_CustomStep0_UserValue=|DC_PrimaryStart_UserValue=|DC_PrimaryStop_UserValue=|DC_PrimaryStep_UserValue=|ParamSweep_CustomStart1_UserValue=|ParamSweep_CustomStop1_UserValue=|ParamSweep_CustomStep1_UserValue=100pF|ParamSweep_Start2_UserValue=|ParamSweep_Stop2_UserValue=|OPTION_ITL4=100|ParamSweep_CustomStart2_UserValue=|ParamSweep_CustomStop2_UserValue=|DC_CustomEnabled0=True|DC_CustomSource0=IC1A|DC_CustomStart0=1n|DC_CustomStop0=1u|DC_CustomStep0=100n|TRAN_VariableEnabled0=True|TRAN_XVariable0=|TRAN_Variable0=v(U_SQR)|TRAN_VariableName0=U_SQR|TRAN_VariableUnits0=V|TRAN_VariablePlot0=1|TRAN_VariableAxis0=0|TRAN_VariableColor0=8421504|TRAN_VariableEnabled1=True|TRAN_XVariable1=|TRAN_Variable1=v(U_TRI)|TRAN_VariableName1=U_TRI|TRAN_VariableUnits1=V|TRAN_VariablePlot1=0|TRAN_VariableAxis1=0|TRAN_VariableColor1=8421504|TRAN_VariableEnabled2=True|TRAN_XVariable2=|TRAN_Variable2=v(U_SQR_OTA)-v(U_TRI)|TRAN_VariableName2=Delta-V @ OTA-B|TRAN_VariableUnits2=V|TRAN_VariablePlot2=2|TRAN_VariableAxis2=0|TRAN_VariableColor2=8421504|TRAN_VariableEnabled3=True|TRAN_XVariable3=|TRAN_Variable3=v(R_lambda_T)|TRAN_VariableName3=U_lambda_T|TRAN_VariableUnits3=V|TRAN_VariablePlot3=3|TRAN_VariableAxis3=0|TRAN_VariableColor3=8421504|TRAN_VariableEnabled4=True|TRAN_XVariable4=|TRAN_Variable4=i(U_mess)|TRAN_VariableName4=I_ABC|TRAN_VariableUnits4=A|TRAN_VariablePlot4=4|TRAN_VariableAxis4=0|TRAN_VariableColor4=8421504|TRAN_VariableEnabled5=True|TRAN_XVariable5=|TRAN_Variable5=v(U_C)|TRAN_VariableName5=U_C|TRAN_VariableUnits5=V|TRAN_VariablePlot5=3|TRAN_VariableAxis5=0|TRAN_VariableColor5=8421504|TRAN_VariableEnabled6=True|TRAN_XVariable6=|TRAN_Variable6=i(U_messref)|TRAN_VariableName6=I_ref + I_ABC|TRAN_VariableUnits6=A|TRAN_VariablePlot6=4|TRAN_VariableAxis6=0|TRAN_VariableColor6=8421504|TRAN_VariableEnabled7=True|TRAN_XVariable7=|TRAN_Variable7=v(U_SAW)|TRAN_VariableName7=U_SAW|TRAN_VariableUnits7=V|TRAN_VariablePlot7=5|TRAN_VariableAxis7=0|TRAN_VariableColor7=8421504|AC_VariableEnabled0=True|AC_XVariable0=|AC_Variable0=MAG(v(U_TRI))|AC_VariableName0=|AC_VariableUnits0=|AC_VariablePlot0=0|AC_VariableAxis0=0|AC_VariableColor0=8421504|Variable0=MAG(v(U_TRI))|VariablePlot0=0|VariableAxis0=0|VariableName0=|VariableUnits0=|VariableColor0=8421504|ParamSweep_CustomEnabled0=False|ParamSweep_CustomParameter0=U_var|ParamSweep_CustomType0=LIST|ParamSweep_CustomStart0=1|ParamSweep_CustomStop0=5|ParamSweep_CustomStep0=1 1.083 1.166 1.25 1.333 1.416 1.5 1.583 1.666 1.75 1.833 1.916|ParamSweep_CustomEnabled1=True|ParamSweep_CustomParameter1=R_ref|ParamSweep_CustomType1=LIST|ParamSweep_CustomStart1=|ParamSweep_CustomStop1=|ParamSweep_CustomStep1=1.6905Meg|ParamSweep_CustomEnabled2=True|ParamSweep_CustomParameter2=U_var|ParamSweep_CustomType2=LIST|ParamSweep_CustomStart2=|ParamSweep_CustomStop2=|ParamSweep_CustomStep2=1.08333|Sensitivity_ParameterEnabled0=True|Sensitivity_Parameter0=Temp|Sensitivity_ParameterDeviation0=1m</Config>
          <Charts>
            <ChartConfig>
              <Name>AC Analysis</Name>
              <Id>OGOYUJKI</Id>
            </ChartConfig>
          </Charts>
        </ResultConfig>
      </Results>
    </DocumentConfig>
  </Documents>
  <Results />
</ProjectConfig>