<?xml version="1.0" encoding="utf-8"?><!DOCTYPE eagle SYSTEM "eagle.dtd"><eagle version="9.7.0"><drawing><board><plain><wire x1="0" y1="0" x2="112.47500000000001" y2="0" width="0" layer="20"/><wire x1="112.47500000000001" y1="0" x2="112.47500000000001" y2="56.03999999999998" width="0" layer="20"/><wire x1="112.47500000000001" y1="56.03999999999998" x2="0" y2="56.03999999999998" width="0" layer="20"/><wire x1="0" y1="56.03999999999998" x2="0" y2="0" width="0" layer="20"/></plain><libraries><library name="Tinkercad"><packages><package name="RESAD1016W63L850D250B"><description>Axial Resistor, 10.16 mm pitch, 8.50 mm body length, 2.50 mm body diameter &lt;p&gt;Axial Resistor package with 10.16 mm pitch (lead spacing), 0.63 mm lead diameter, 8.50 mm body length and 2.50 mm body diameter&lt;/p&gt;</description></package><package name="DIP762W53P254L1969H508Q16B"><description>16-DIP, 2.54 mm (0.10 in) pitch, 7.62 mm (0.30 in) span, 19.69 X 6.6 X 5.08 mm body&lt;p&gt;16-pin DIP package with 2.54 mm (0.10 in) pitch, 7.62 mm (0.30 in) span with body size 19.69 X 6.6 X 5.08 mm&lt;/p&gt;</description></package><package name="CAP-THRU-2.54MM"></package></packages></library></libraries><attributes/><variantdefs/><elements><element name="R3" library="Tinkercad" package="RESAD1016W63L850D250B" value="1k"/><element name="R1" library="Tinkercad" package="RESAD1016W63L850D250B" value="10k"/><element name="C3" library="Tinkercad" package="CAP-THRU-2.54MM" value="1n"/><element name="C2" library="Tinkercad" package="CAP-THRU-2.54MM" value="1n"/><element name="R4" library="Tinkercad" package="RESAD1016W63L850D250B" value="1k"/><element name="R7" library="Tinkercad" package="RESAD1016W63L850D250B" value="22k"/><element name="R5" library="Tinkercad" package="RESAD1016W63L850D250B" value="1k"/><element name="R2" library="Tinkercad" package="RESAD1016W63L850D250B" value="22k"/><element name="R8" library="Tinkercad" package="RESAD1016W63L850D250B" value="1k"/><element name="R6" library="Tinkercad" package="RESAD1016W63L850D250B" value="5k"/><element name="U1" library="Tinkercad" package="DIP762W53P254L1969H508Q16B" value="L293E"/><element name="R9" library="Tinkercad" package="RESAD1016W63L850D250B" value="5k"/><element name="R12" library="Tinkercad" package="RESAD1016W63L850D250B" value="470"/><element name="U2" library="Tinkercad" package="DIP762W53P254L1969H508Q16B" value="L293E"/><element name="R13" library="Tinkercad" package="RESAD1016W63L850D250B" value="3k"/><element name="C4" library="Tinkercad" package="CAP-THRU-2.54MM" value="220n"/><element name="R14" library="Tinkercad" package="RESAD1016W63L850D250B" value="27k"/><element name="R11" library="Tinkercad" package="RESAD1016W63L850D250B" value="470"/><element name="R15" library="Tinkercad" package="RESAD1016W63L850D250B" value="5k"/><element name="C5" library="Tinkercad" package="CAP-THRU-2.54MM" value="220n"/><element name="R16" library="Tinkercad" package="RESAD1016W63L850D250B" value="56k"/><element name="R10" library="Tinkercad" package="RESAD1016W63L850D250B" value="22k"/></elements><signals><signal name="U1_4Y"><contactref element="R1" pad="1"/><contactref element="U1" pad="14"/><contactref element="R3" pad="1"/><contactref element="C2" pad="1"/><contactref element="R5" pad="2"/><contactref element="C3" pad="2"/><contactref element="R4" pad="2"/><contactref element="R12" pad="1"/><contactref element="R11" pad="1"/><contactref element="R14" pad="1"/></signal><signal name="U1_GND4"><contactref element="U1" pad="12"/><contactref element="C2" pad="2"/><contactref element="U1" pad="10"/><contactref element="U1" pad="5"/><contactref element="C3" pad="1"/><contactref element="U1" pad="7"/><contactref element="U1" pad="4"/><contactref element="R8" pad="2"/><contactref element="U1" pad="13"/><contactref element="R7" pad="2"/><contactref element="R4" pad="1"/></signal><signal name="U1_3-4EN"><contactref element="U1" pad="9"/><contactref element="R2" pad="1"/><contactref element="R6" pad="1"/><contactref element="R7" pad="1"/></signal><signal name="U1_1Y"><contactref element="R2" pad="2"/><contactref element="R5" pad="1"/><contactref element="U1" pad="3"/></signal><signal name="U2_2Y"><contactref element="U2" pad="6"/><contactref element="R10" pad="1"/><contactref element="R9" pad="1"/><contactref element="R8" pad="1"/><contactref element="R6" pad="2"/><contactref element="U1" pad="6"/><contactref element="R15" pad="1"/><contactref element="R16" pad="1"/></signal><signal name="U1_3Y"><contactref element="U1" pad="11"/><contactref element="U2" pad="11"/></signal><signal name="U1_1-2EN"><contactref element="U1" pad="1"/><contactref element="U1" pad="16"/></signal><signal name="U1_VCC2"><contactref element="U1" pad="8"/><contactref element="R9" pad="2"/></signal><signal name="U2_1Y"><contactref element="U2" pad="3"/><contactref element="R12" pad="2"/><contactref element="R13" pad="2"/></signal><signal name="U2_GND1"><contactref element="U2" pad="4"/><contactref element="R11" pad="2"/><contactref element="U2" pad="5"/><contactref element="R14" pad="2"/><contactref element="U2" pad="7"/><contactref element="R15" pad="2"/><contactref element="C5" pad="1"/><contactref element="U2" pad="12"/><contactref element="U2" pad="13"/></signal><signal name="R13_1"><contactref element="R13" pad="1"/><contactref element="C4" pad="1"/></signal><signal name="C5_2"><contactref element="C5" pad="2"/><contactref element="R16" pad="2"/></signal></signals></board></drawing></eagle>